Netgear R7800
	Use TFTP method with ROOter factory image

	Router IP Address   - 192.168.1.1
	Computer IP Address - 192.168.1.10
	White Led should flash about 10 times before releasing reset.
	
Asus RT-AC51U
Asus RT-AC56U
Asus RT-AC68U
Asus RT-AC87U
Asus RT-N66U
	Use TFTP method with ROOter factory image

	Router IP Address   - 192.168.1.1
	Computer IP Address - 192.168.1.10
	
Asus RT-AC56U
	Details - https://openwrt.org/toh/asus/rt-ac58u#installation
	
