Use the uboot recovery GUI to flash from Factory to ROOter.

Unplug power, hold down the reset button and plug in power.

Led will flash 5 times then go solid white. Release reset button.

Go to 192.168.1.1 and flash using the UBI file.

Use the BIN file when updating from the ROOter GUI.