
Archer A7v5
	Use TFTP method with ROOter factory image

	Router IP Address   - 192.168.0.66
	Computer IP Address - 192.168.0.86
	Firmware name 		- ArcherC7v5_tp_recovery.bin

Archer C7v1
	Factory Gui with ROOter factory image
	Firmware name		- c7v1.bin
		
Archer C7v2
	Factory Gui with ROOter factory image
	Firmware name		- c7v2.bin
	
Archer C7v4
	Use TFTP method with ROOter factory image

	Router IP Address   - 192.168.0.66
	Computer IP Address - 192.168.0.86
	Firmware name 		- ArcherC7v4_tp_recovery.bin
	
Archer C7v5
	Use TFTP method with ROOter factory image

	Router IP Address   - 192.168.0.66
	Computer IP Address - 192.168.0.86
	Firmware name 		- ArcherC7v5_tp_recovery.bin

MR3020v3
	Use TFTP method with ROOter factory image

	Router IP Address   - 192.168.0.66
	Computer IP Address - 192.168.0.225
	Firmware name 		- tp_recovery.bin
	
MR3420v5
	Use TFTP method with ROOter factory image

	Router IP Address   - 192.168.0.66
	Computer IP Address - 192.168.0.225
	Firmware name 		- tp_recovery.bin
	
WR942v1
	Use TFTP method with ROOter factory image

	Router IP Address   - 192.168.0.86
	Computer IP Address - 192.168.0.66
	Firmware name 		- WR942v1_recovery.bin

WR842v3
	Use TFTP method with ROOter factory image

	Router IP Address   - 192.168.0.86
	Computer IP Address - 192.168.0.66
	Firmware name 		- wr842nv3_tp_recovery.bin

WDR3500
	Factory Gui with ROOter factory image
	Firmware name		- wdr3500v1_tp_recovery.bin
	
WDR3600
	Factory Gui with ROOter factory image
	Firmware name		- wdr3600v1_tp_recovery.bin

WDR4300
	Factory Gui with ROOter factory image
	Firmware name		- wdr4300v1_en_3_14_3_up_boot(150518).bin	

WDR4310
	Factory Gui with ROOter factory image
	
WR902ACv1
	Factory Gui with ROOter factory image
	Firmware name		- update.bin	

WR903ACv3
	Use TFTP method with ROOter factory image

	Router IP Address   - 192.168.0.86
	Computer IP Address - 192.168.0.66
	Firmware name 		- tp_recovery.bin

WR1043NDv2
	Factory Gui with ROOter factory image
	Firmware name		- firmware.bin	
	
WR1043NDv3
	Factory Gui with ROOter factory image
	Firmware name		- firmware.bin	
		
C20v1
	Factory Gui with ROOter factory image
	Details - https://openwrt.org/toh/tp-link/archer_c20i

C2v1
	Details - https://openwrt.org/toh/tp-link/archer_c2_ac750

C6Uv1
	Factory Gui with ROOter factory image

	
